**Carleton University**

**Department of Systems and Computer Engineering**

**SYSC 3006 (Computer Organization) summer 2020**

**Lab / Assignment 3– Answers file**

Student Name: ID#:

### Part 1 – [2.4-mark/5]

### 1-1

1. [0.50-mark] Fill in the Part 1 Instruction Encoding Table for the following instructions.

|  |  |  |
| --- | --- | --- |
| OPR | Instruction | Encoding (hex) |
| NOT | R5 ← NOT R4 |  |
| SUB | R7 ← R6 – R5 |  |
| NOP | NOP |  |
| MOV | R0 ← R7 |  |

1. [0.50-mark] Complete the FSM Output ROM for part 1.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | **3 1** | **3 0** | **2 9** | **2 8** | **2 7** | **2 6** | **2 5** | **2 4** | **2 3** | **2 2** | **2 1** | **2 0** | **1 9** | **1 8** | **1 7** | **1 6** | **1 5** | **1 4** | **1 3** | **1 2** | **1 1** | **1 0** | **9** | **8** | **7** | **6** | **5** | **4** | **3** | **2** | **1** | **0** |  |
| **State**  **Hex encoding** | **Unused (0)** | **IRCE** | **PCOE** | **C1OE** | **AADD** | **MARCE** | **MAROE** | **MDRCE** | **MDROE** | **MDRget** | **MDRput** | **IBRead** | **IBWrite** | **AOP** | **ANOP** | **DR** | **SXR** | **SYR** | **RegSEL** | **RegLD** | **T1CE** | **T1OE** | **T2CE** | **T2OE** | **Q7+** | **Q6+** | **Q5+** | **Q4+** | **Q3+** | **Q2+** | **Q1+** | **Q0+** | **Hex**  **Encoding** |
| **F0**  **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **1** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **1** | **0002 0001** |
| **F1**  **1** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **1** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **1** | **0** | **0002 0002** |
| **F2**  **2** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **1** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **1** | **1** | **0002 0003** |
| **Decode**  **3** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** |  |  |  |  |  |  |  |  |  |  |  | **0** | **0** | **0** | **0** | **0** | **1** | **1** | **1** | **000x xx07** |
| **E0**  **4** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** |  |  |  |  |  |  |  |  |  |  |  | **0** | **0** | **0** | **0** | **0** | **1** | **0** | **1** | **000x xx05** |
| **E1**  **5** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** |  |  |  |  |  |  |  |  |  |  |  | **0** | **0** | **0** | **0** | **0** | **1** | **1** | **0** | **000x xx06** |
| **E2**  **6** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** |  |  |  |  |  |  |  |  |  |  |  | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **000x xx00** |
| **Dead**  **7** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **1** | **1** | **1** | **000x xx07** |

1. [0.50-mark] Complete the FSM Decode ROM Tables (this table is same for Part 1 and 2 of this lab).

|  |  |  |
| --- | --- | --- |
| Instruction | Address  (hex) | Contents  (hex) |
| NOP | 00 |  |
| ADD | 01 | **04** |
| SUB | 02 |  |
| MOV | 03 |  |
| AND | 04 |  |
| OR | 05 |  |
| XOR | 06 |  |
| NOT | 07 |  |

NOTE: In the supplied circuit, the Control FSM outputs the RegSEL and RegLD signals with the behaviour expected by the Registers RAM. The FSM Output ROM does not use RegR and RegW signals as done in Lab‐II and in class; the RegSEL and RegLD signals (with Logisim RAM signaling behaviour) are used instead.

Do not change any of the values that have been pre‐entered into the table, except for the empty cases in the hexadecimal encodings (in Part 1 FSM Output ROM Table). The first 3 states are there only as placeholders in Part 1 and have been designed to have no undesirable effects on the circuit. This allows you to always start the FSM in state 0.

The resulting FSM Output ROM and FSM Decode ROM values should work for any of the instructions discussed in class that use the ALU (i.e. NOP, ADD, SUB, MOV, AND, OR, XOR and NOT).

1. [0.50-mark] Save your circuit as Lab‐3\_Part1.circ. and submit it with your assignment for verification and to get the marks for this section.
2. [0.40-mark] Same as you did in lab 2, execute the instructions in the table above in the given sequence with all registers initially containing 0x0. Log the execution of the sequence on your implementation to validate the execution of the required instructions and show the results here. (The simulation log should include: Current State, IR, PC, registers, and Next State. Set the log radix to hex).

### Part 2 – [total of 2.6-mark/5]

### 2.1 - Tables

1. [0.50-mark] Complete the Part 2 FSM Output ROM Table.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | **3 1** | **3 0** | **2 9** | **2 8** | **2 7** | **2 6** | **2 5** | **2 4** | **2 3** | **2 2** | **2 1** | **2 0** | **1 9** | **1 8** | **1 7** | **1 6** | **1 5** | **1 4** | **1 3** | **1 2** | **1 1** | **1 0** | **9** | **8** | **7** | **6** | **5** | **4** | **3** | **2** | **1** | **0** |  |
| **State**  **Hex encoding** | **Unused (0)** | **IRCE** | **PCOE** | **C1OE** | **AADD** | **MARCE** | **MAROE** | **MDRCE** | **MDROE** | **MDRget** | **MDRput** | **IBRead** | **IBWrite** | **AOP** | **ANOP** | **DR** | **SXR** | **SYR** | **RegSEL** | **RegLD** | **T1CE** | **T1OE** | **T2CE** | **T2OE** | **Q7+** | **Q6+** | **Q5+** | **Q4+** | **Q3+** | **Q2+** | **Q1+** | **Q0+** | **Hex**  **Encoding** |
| **F0**  **0** | **0** |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **1** |  |
| **F1**  **1** | **0** |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | **0** | **0** | **0** | **0** | **0** | **0** | **1** | **0** |  |
| **F2**  **2** | **0** |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | **0** | **0** | **0** | **0** | **0** | **0** | **1** | **1** |  |
| **Decode**  **3** | **0** |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | **0** | **0** | **0** | **0** | **0** | **1** | **1** | **1** |  |
| **E0**  **4** | **0** |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | **0** | **0** | **0** | **0** | **0** |  |  |  |  |
| **E1**  **5** | **0** |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | **0** | **0** | **0** | **0** | **0** |  |  |  |  |
| **E2**  **6** | **0** |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** |  |
| **Dead**  **7** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **0** | **1** | **1** | **1** | **0000 0007** |

1. [0.40-mark]Complete the Part 2 Main Memory Instructions Table for the following instructions.

|  |  |  |
| --- | --- | --- |
| Instruction | Address (hex) | Contents (hex) |
| R10 ← R1 OR R2 | 00 |  |
| R11 ← R2 – R10 | 01 |  |
| R12 ← NOT (R11) | 02 |  |
| R13 ← R0 + R12 | 03 |  |

### 2.2 - Circuit wiring

Save a copy of your part 1 (Save as) and name it “Lab3-Part-2.circ”. Then extend your Processor solution to Part 1 to read and execute instructions from Main Memory. You will not need to modify the circuit beyond the description of modifications given above.

1. [0.30-mark] Show below a screenshot of the new control FMS outputs that you added in the Logisim circuits, and a short description about each output.
2. [0.40-mark] Show here a screenshot of the new hardware components that you added in the Logisim circuits. Include a short description about each component function.
3. [0.30-mark] Include a copy of your Lab3-Part-2.circ circuit with your submission. We must verify your circuit functionality in order to assign you marks for this part (c)

### 2.3 Execution test

1. [0.40-mark] The Part 2 Main Memory Instructions Table in 2.1 –b) contain same instruction sequence from your lab 2-part 2, but here they are encoded over 32-bit word width. Clear the 16 internal register bloc and the Main memory to 0x0. Then as you did in lab 2, initiate R0 to 0x00000001, R1 to 0x1000000F and R2 to 0xF0000000. Then insert the instructions from the Table in 2.1 –b) above into the Main Memory starting at address 0 and up (one instruction per address word as indicated in the table) in the given sequence. Now, execute all the instructions (repeat fetch-decode-execute cycle till all instruction are fully executed). To execute all instruction just poke the Toggle Switch to advance the FSM through the operation till all instructions are fully executed (while observing their execution). Make sure you PC (R15), holds the address of the first instruction to be fetched, then observe it increments… to fetch the next... Same as you did in part 1, log the execution of the sequence on your implementation to validate the execution of the required instructions and show the results here.
2. [0.30-mark] Compare the concept used here to your lab 2-part 2, briefly describe here what is the advantage of the concept here over lab2-part 2?

# Submission deadline

Must be submitter on cuLearn, locate (Assignment 3 submission) and follow instructions. Submission exact deadline (date and time) is displayed clearly within the Assignment 3 submission on cuLearn.

***Note: If you have any question please contact your respective group TA (see TA / group information posted on cuLearn) or use Discord class server.***

Good Luck